Main Page Namespace List Compound List File List Namespace Members Compound Members

# nFANTOM100::iNXT Member List

This is the complete list of members for nFANTOM100::iNXT, including all inherited members.

- bluetoothFactoryReset(tStatus &status)=0 `[pure virtual]`
- bootIntoFirmwareDownloadMode(tStatus &status)=0 `[pure virtual]`
- createFile(ViConstString fileName, tStatus &status)=0 `[pure virtual]`
- createFileIterator(ViConstString fileNamePattern, tStatus &status)=0 `[pure virtual]`
- createModule(ViConstString moduleName, ViUInt32 moduleID, ViUInt32 moduleSizeInBytes, ViUInt32 ioMapSizeInBytes, tStatus &status)=0 `[pure virtual]`
- createModuleIterator(ViConstString moduleNamePattern, tStatus &status)=0 `[pure virtual]`
- createNXT(ViConstString resourceString, tStatus &status, ViBoolean checkFirmwareVersion=true) `[static]`
- createNXTIterator(ViBoolean searchBluetooth, ViUInt32 bluetoothSearchTimeoutInSeconds, tStatus &status) `[static]`
- destroyFile(iFile *filePtr)=0 `[pure virtual]`
- destroyFileIterator(iFileIterator *fileIteratorPtr)=0 `[pure virtual]`
- destroyModule(iModule *modulePtr)=0 `[pure virtual]`
- destroyModuleIterator(iModuleIterator *moduleIteratorPtr)=0 `[pure virtual]`
- destroyNXT(iNXT *nxtPtr) `[static]`
- destroyNXTIterator(iNXTIterator *iterPtr) `[static]`
- downloadFirmware(const ViByte firmwareBufferPtr[], ViUInt32 firmwareBufferSizeInBytes, tStatus &status)=0 `[pure virtual]`
- eraseUserFlash(tStatus &status)=0 `[pure virtual]`
- findDeviceInFirmwareDownloadMode(ViChar resourceName[], tStatus &status) `[static]`
- getDeviceInfo(ViChar name[], ViByte bluetoothAddress[], ViUInt8 signalStrength[], ViUInt32 &availableFlash, tStatus &status)=0 `[pure virtual]`
- getFirmwareVersion(ViUInt8 &protocolVersionMajorRef, ViUInt8 &protocolVersionMinorRef, ViUInt8 &firmwareVersionMajorRef, ViUInt8 &firmwareVersionMinorRef, tStatus &status)=0 `[pure virtual]`
- getResourceString(ViChar resourceString[], tStatus &status)=0 `[pure virtual]`
- isPaired(ViConstString resourceName, tStatus &status) `[static]`
- kBufferHighSpeed enum value (defined in nFANTOM100::iNXT)
- kBufferStandard enum value (defined in nFANTOM100::iNXT)
- pairBluetooth(ViConstString resourceName, ViConstString passkey, ViChar pairedResourceName[], tStatus &status) `[static]`
- pollAvailableLength(tBuffer bufferSelector, tStatus &status)=0 `[pure virtual]`
- read(ViPBuf bufferPtr, ViUInt32 numberOfBytes, tStatus &status)=0 `[pure virtual]`
- readBufferData(ViPBuf dataBuffer, tBuffer bufferSelector, ViUInt32 numberOfBytesToRead, tStatus &status)=0 `[pure virtual]`
- sendDirectCommand(ViBoolean requireResponse, const ViByte commandBufferPtr[], ViUInt32 commandBufferSizeInBytes, ViPBuf responseBufferPtr, ViUInt32 responseBufferSizeInBytes, tStatus &status)=0 `[pure virtual]`
- setName(ViConstString newName, tStatus &status)=0 `[pure virtual]`
- tBuffer enum name
- unpairBluetooth(ViConstString resourceName, tStatus &status) `[static]`
- write(const ViByte bufferPtr[], ViUInt32 numberOfBytes, tStatus &status)=0 `[pure virtual]`
- ~iNXT()=0 `[protected, pure virtual]`

© Copyright 2005-2006, National Instruments Corporation. All rights reserved.